NOTIFICATION

The following notification is being circulated in accordance with Article 10.6.

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** CHILE**If applicable, name of local government involved (Articles 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** *Ministerio de Obras Públicas*, MOP (Ministry of Public Works)**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:***Dirección General de Relaciones Económicas Internacionales* - *Ministerio de Relaciones Exteriores* (Directorate-General of International Economic Relations, Ministry of Foreign Affairs) |
| **3.** | **Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Carbon steel bar grating, grating for flooring and steps |
| **5.** | **Title, number of pages and language(s) of the notified document:** *NCh 3572 Parrillas de barras de acero al carbono - Parrillas de piso y peldaños - Requisitos para su fabricación y uso* (Chilean Standard (NCh) No. 3572, Carbon steel bar grating - Grating for flooring and steps - Requirements for manufacturing and use) (60 pages, in Spanish)  |
| **6.** | **Description of content:** The notified Standard establishes the classification and description of floor and step grating used for industrial floors, steps, platforms, gangways, drainage channels, etc.It establishes geometrical and dimensional requirements and tolerances for grating for flooring and steps.It also establishes the mechanical, chemical composition and dimensional requirements to be met by carbon steel bars (primary material) used to manufacture grating for flooring and steps. It furthermore contains calculation tables for the design of such products.The notified Standard establishes the requirements for the volume calculation, manufacture and delivery of grating for flooring and steps.It does not apply to grating steps made from materials other than steel and carbon, or manufactured using different manufacturing methods, such as pressure-locked and/or riveted grating |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Quality requirements |
| **8.** | **Relevant documents:** *NCh 3572 Parrillas de barras de acero al carbono - Parrillas de piso y peldaños - Requisitos para su fabricación y uso* (Chilean Standard (NCh) No. 3572, Carbon steel bar grating - Grating for flooring and steps - Requirements for manufacturing and use)  |
| **9.** | **Proposed date of adoption:** -**Proposed date of entry into force:** - |
| **10.** | **Final date for comments:** 60 days from the date of notification |
| **11.** | **Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body:***Departamento Regulatorio* (Regulations Department)*Dirección General de Relaciones Económicas Internacionales* (Directorate-General of International Economic Relations)*Ministerio de Relaciones Exteriores* (Ministry of Foreign Affairs)Teatinos 180, piso 11Tel.: (+56) 2-22827 5250Fax: (+56) 2-22380 9494Email: tbt\_chile@direcon.gob.clNote: To view the above-mentioned Chilean Standard, go to <https://www.inncoleccion.cl/> and enter the following data:Company: DIRECON-020Username: direconPassword: direconEmail: tbt\_chile@direcon.gob.cl  |